1.a) input 50mV and 1kHz for (10k and 100k)





b) frequency response





2. a) input 50mV and 1kHz for (10k and 22k)





b) frequency response





3. input 100mV and 50kHz

a) 10k and 100k





Frequency response



b) 10k and 22k





Frequency response

