2. Setting voltage at C





Voltage at C = 5V



3. Differential mode (potentiometer at minimum value – maximum gain)





Output voltage (Pin 6 of U3)



4. Common mode



Output voltage (Pin 6 of U3)





6. Differential mode (potentiometer at maximum value 47k – minimum gain)





